<?xml version="1.0" encoding="utf-8" standalone="no"?>
<!DOCTYPE article PUBLIC "-//OASIS//DTD DocBook XML V4.1.2//EN" "http://www.oasis-open.org/docbook/xml/4.1.2/docbookx.dtd" [
<!ENTITY app "Ekiga">
<!ENTITY appversion "4.0">
<!ENTITY manrevision "4.0">
]>
<!-- Begin -->
<article id="index" lang="sv">
<articleinfo>
<title><application>Ekiga</application> Manual 4.0 </title>

<copyright><year>2003-2012</year><holder>Damien Sandras</holder></copyright>
<copyright><year>2003-2004</year><holder>Matthias Redlich</holder></copyright>
<copyright><year>2003-2004</year><holder>Christopher Warner</holder></copyright><copyright><year>2006, 2007, 2008</year><holder>Daniel Nylander (po@danielnylander.se)</holder></copyright>
<!-- translators: uncomment this:

<copyright>
<year>2002</year>
<holder>ME-THE-TRANSLATOR (Latin translation)</holder>
</copyright>

-->

<revhistory>
<revision>
<revnumber>Ekiga Manual 4.0</revnumber>
<date>2012-06-03</date>
<revdescription>
<para role="author">Damien Sandras</para>
</revdescription>
</revision>
<revision>
<revnumber>Handbok för Ekiga 3.0</revnumber>
<date>2008-08-31</date>
<revdescription>
<para role="author">Damien Sandras</para>
</revdescription>
</revision>
<revision>
<revnumber>Handbok för Ekiga 2.0</revnumber>
<date>2006-01-22</date>
</revision>
</revhistory>

<publisher>
<publishername>Damien Sandras</publishername>
<address><email>dsandras@seconix.com</email></address>
</publisher>
<publisher>
<publishername>Christopher Warner</publishername>
<address><email>zanee@kernelcode.com</email></address>
</publisher>
<publisher>
<publishername>Matthias Redlich</publishername>
<address><email>m-redlich@t-online.de</email></address>
</publisher>

<authorgroup>
<author role="maintainer">
<firstname>Damien</firstname>
<surname>Sandras</surname>
</author>
<author>
<firstname>Christopher</firstname>
<surname>Warner</surname>
<othername>zanee</othername>
</author>
<author>
<firstname>Matthias</firstname>
<surname>Redlich</surname>
</author>
</authorgroup>

<releaseinfo>
This documentation is for version 4.0 of Ekiga.
</releaseinfo>

<abstract role="description">
<para>Ekiga är ett program för röstsamtal över IP, IP-telephoni och videokonferenser, med stöd för många ljud- och videokodekar.</para>
</abstract>
</articleinfo>

<indexterm zone="index">
<primary>Ekiga</primary>
</indexterm>
<indexterm zone="index">
<primary>Ekiga</primary>
</indexterm>
<indexterm zone="index">
<primary>Ekiga</primary>
</indexterm>

<!-- INTODUCTION          -->
<!-- What is &app; -->

<section id="ekiga-introduction">
<title>Introduktion</title>

<section><title>Ekiga</title>
<para><application>Ekiga</application> är ett program för fri Voice over IP, IP-telefoni och videokonferenser för Linux och andra dialekter (t.ex. BSD, OpenSolaris eller MacOSX). Det skrevs av Damien Sandras och är licenserat under GNU/GPL.</para>

<para>Ekiga kan använda moderna "Voice over IP"-protokoll som SIP och H.323. Det har stöd för alla större funktioner som definierats av dessa protokoll  som <emphasis>samtalsparkering</emphasis>, <emphasis>koppling av samtal</emphasis>, <emphasis>vidarekoppling av samtal</emphasis>, ... Det har även grundläggande stöd för <emphasis>snabbmeddelanden</emphasis> och <emphasis>närvaro</emphasis>. Det har även avancerat stöd för <emphasis>NAT-traversering</emphasis>. Ekiga har stöd för de bästa <emphasis>fria</emphasis> ljud- och videokodekarna och har "wideband"-stöd för en överlägsen ljudkvalitet, tillsammans med ekosläckning.</para>
</section>

<section><title>SIP och H.323</title>
<para>Session Initiation Protocol (SIP) är ett protokoll som utvecklats av IETF MMUSIC Working Group och är en föreslagen standard för initiering, ändring, och terminering av en interaktiv användarsession som involverar multimediaelement såsom video, röst, snabbmeddelanden, nätverksspel, och virtual verklighet. I november 2000 blev SIP accepterad som ett 3GPP-signalprotokoll och permanent element för IMS-arkitekturen. Det är ett av de ledande signalprotokollet för "Voice over IP" (röst över IP).</para>

<para>H.323 blev ursprungligen skapad för att tillhandahålla en mekanism för att transportera  multimediaprogram över lokala nätverk, men har snabbt växt till att möta det växande behovet för VoIP-nätverk. En styrka hos H.323 var den relativa tillgängligheten av standarder, inte bara de som definierade den grundläggande samtalsmodellen, men även ytterligare tjänster, behovet av att möta förväntningarna för affärskommunikation. H.323 var den fösta VoIP-standarden att använda IETF-standarden RTP för att transportera ljud och video över IP-nätverk. H.323 är baserad på protokollet ISDN Q.931 som lämpar sig för scenarier där IP och ISDN samarbetar, även mellan IP och QSIG. En samtalsmodell, liknande  samtalsmodellen för ISDN, gör introduktionen av IP-telefoni in i existerande nätverk med ISDN-baserade telefonväxelsystem enklare.</para>
<para>
<graphic fileref="figures/lumi.png"/>
</para>
</section>
</section>

<section id="ekiga-getting-started">
<title>Komma igång</title>
<para>När <application>Ekiga</application> startas för första gången kommer konfigurationsguiden att visas automatiskt. Konfigurationsguiden är en steg-för-steg-guide som hjälper dig genom alla steg som krävs för att skapa den grundläggande konfigurationen som du behöver för att kunna använda <application>Ekiga</application>. Du bör gå genom dessa steg grundligt, annars kommer guiden att dyka upp igen (när den inte har färdigställts) eller så kommer inte <application>Ekiga</application> att fungera korrekt (om några av dina svar inte har rättats till). Du kan köra konfigurationsguiden när som helst från Redigera-menyn.</para>

<tip><title>Tips</title><para>Alla inställningar kan ändras via inställningsfönstret när som helst.</para></tip>


<section><title>Introduktion till konfigurationsguiden</title>
<figure>
<title/>
<graphic fileref="figures/config_d1.png"/>
</figure>

<para>Navigering finns tillgänglig i nederkant av fönstret genom hela konfigurationsprocessen. Du kommer att kunna navigera genom frågorna med Bakåt, Framåt och Avbryt. Om du trycker på Avbryt under konfigurationen kommer <application>Ekiga</application> inte att påverkas av dina ändringar och all inmatad information kommer att förkastas.</para>

<para>Den här sidan välkomnar dig till konfigurationsguiden. Det finns ingenting att ändra eller redigera här. Tryck på "Framåt"-knappen i nederkant av fönstret för att påbörja konfigurationen.</para>
</section>


<section><title>Personlig information</title>
<figure>
<title/>
<graphic fileref="figures/config_d2.png"/>
</figure>

<para>Fönstret för Personlig information kräver att du matar in personlig information som ska användas i <application>Ekiga</application>. Den här informationen visas vid anslutning till andra ljud-/videoprogram.</para>
</section>


<section><title>Accounts</title>
<figure>
<title/>
<graphic fileref="figures/config_d3.png"/>
</figure>

<para>
The Accounts window gives you a clear explanation of what accounts are for. You may simply skip it if you already know what an account is and what to use it for.
</para>
</section>


<section><title>Ekiga.net-konto</title>
<figure>
<title/>
<graphic fileref="figures/config_d4.png"/>
</figure>

<para>Ekiga.net är en fri SIP-tjänstplattform som tillhandahålls för <application>Ekiga</application>-användare. Om du vill ringa andra användare och själv bli uppringd så behöver du en SIP-adress. Du kan få en från <ulink url="http://www.ekiga.net" type="http">http://www.ekiga.net</ulink>. Ekiga.net erbjuder även ytterligare tjänster som konferensrum, röstbrevlåda eller telefonkatalogtjänst. Se <ulink url="http://www.ekiga.net" type="http">http://www.ekiga.net</ulink> för mer information.</para>

<para>Följ helt enkelt länken som angivits i dialogrutan för att skaffa ett konto om du inte redan har ett, fyll sedan i ditt användarnamn och lösenord. Tryck på "Framåt" efter att du har matat in all nödvändig information för att fortsätta.</para>
</section>


<section><title>Ekiga Ring ut-konto</title>
<figure>
<title/>
<graphic fileref="figures/config_d5.png"/>
</figure>

<para><application>Ekiga</application> kan användas med flera olika ip-telefonileverantörer. Dessa leverantörer tillåter samtal till riktiga telefoner från din dator med <application>Ekiga</application> mot en samtalsavgift. Vi rekommenderar att du använder standardleverantören i <application>Ekiga</application>.</para>

<para>Om du vill skapa ett konto och använda det för att ringa till dina vänner och familjemedlemmar som har vanliga telefoner mot en samtalsavgift så kan du helt enkelt skapa ett konto med länken "Skaffa ett Ekiga Ring ut-konto". När kontot har skapats så kommer du att få ett inloggningsnamn och lösenord via e-post. Mata helt enkelt in dem i dialogrutan och du är klar att ringa till vanliga telefoner med <application>Ekiga</application></para>

<para>Med standardkonfigurationen så kan du helt enkelt använda sip:3210444555 och välja sip.diamondcard.us för att ringa till det riktiga telefonnumret +3210444555, 32 är landskoden, 10444555 är telefonnumret som ska ringas. Vi rekommenderar att du lägger in dina favorittelefonnummer i adressboken.</para>

<para>Följ helt enkelt länken som angivits i dialogrutan för att skaffa ett konto om du inte redan har ett, fyll sedan i ditt användarnamn och lösenord. Tryck på "Framåt" efter att du har matat in all nödvändig information för att fortsätta.</para>
</section>


<section><title>Anslutningstyp</title>
<figure>
<title/>
<graphic fileref="figures/config_d6.png"/>
</figure>

<para><application>Ekiga</application> har stöd för flera ljud- och videokodekar. Det inkluderar kodekar med mycket bra kvalitet såväl som kodekar med medium till bra kvalitet. Ju högre kvalitet på en kodek, ju mer bandbredd kräver den. Dessutom kan videokodekar justera sin kvalitet till den tillgängliga bandbredden. Detta alternativ är nödvändigt i den initiala konfigurationen av <application>Ekiga</application> så att den kan välja den optimala kodeken som passar din nätverksanslutning och så att den kan justera inställningarna för videokvaliteten. Om din anslutningstyp inte nämns i listan bör du välja den som är närmast din nätverksanslutning och sedan justera <application>Ekiga</application> manuellt i inställningsfönstret (kodeksektionen).</para>

<para>När du är färdig så kan du fortsätta med konfigurationen.</para>
</section>


<section><title>Ljudenheter</title>
<figure>
<title/>
<graphic fileref="figures/config_d7.png"/>
</figure>

<para>
<application>Ekiga</application> requires audio devices to play and record sound. The audio output device ouputs the incoming sound stream during a call. Please select the device that your headset or speakers are connected to. The audio input device is what your microphone is connected to. These settings might be the same as the settings for the audio player if you have only one soundcard. But please note that it is also possible to record sound via another device (e.g. internal microphone in a webcam) too.
This section also allows you to choose the ringing device. This device can be different from the audio output device. It allows you to hear the incoming call ringing sound event in your speakers, while having your headset connected for calls.
</para>

<para>När du är färdig så kan du fortsätta med konfigurationen.</para>
</section>


<section><title>Videoenheter</title>
<figure>
<title/>
<graphic fileref="figures/config_d8.png"/>
</figure>

<para>Det här steget är valfritt och gäller endast för användare som har videoenheter (t.ex. webbkameror). Om du inte har några videoenheter kan du hoppa över den här sidan.</para>

<para>Om du har en webbkamera eller videoenhet som finns i listan kan du välja den här.</para>

<para>När du är färdig så kan du fortsätta med konfigurationen.</para>
</section>


<section><title>Konfigurationen färdig</title>
<figure>
<title/>
<graphic fileref="figures/config_d9.png"/>
</figure>

<para>Konfigurationen av <application>Ekiga</application> är nu färdig. Det sista fönstret visar endast en kort sammanfattning av konfigurationen som du har valt. Verifiera att dessa inställningar är korrekta. Om någonting inte är korrekt kan du använda "Bakåt"-knappen i nederkant av fönstret för att gå till rätt sida i guiden och korrigera felet.</para>

<para>Om allting är korrekt kan du trycka på knappen "Verkställ" för att spara konfigurationen. Guiden kommer då att stängas och huvudfönstret i <application>Ekiga</application> kommer att visas. Kom ihåg att alla inställningar kan ändras när som helst via inställningsfönstret.</para>
</section>

</section>




<section id="ekiga-basic-usage">
<title>Grundläggande användning</title>

<section id="ekiga-calling-and-being-called">
<title>Ring och bli uppringd</title>

<graphic fileref="figures/call_d1.png"/>

<section><title>Från dator till dator (PC-till-PC)</title>
<para>Om du vill ringa andra användare och själv bli uppringd, behöver du en SIP-adress. Du kan få en SIP-adress från <ulink url="http://www.ekiga.net" type="http">http://www.ekiga.net</ulink> som beskrivs här ovanför.</para>

<para>SIP-adressen kan användas av andra användare för att ringa till dig. På samma sätt kan du använda SIP-adressen till dina vänner och familjemedlemmar för att ringa till dem. Du kan till exempel använda <emphasis>sip:dsandras@ekiga.net</emphasis> för att ringa upphovsmannen bakom Ekiga.</para>

<para>Du kan använda online-adressboken för <application>Ekiga</application> för att hitta SIP-adresser till andra användare av <application>Ekiga</application>. Det är så klart möjligt att ringa användare som använder andra leverantörer än ekiga.net. Du kan faktiskt ringa till andra användare som har SIP-programvara eller hårdvara, och som är registrerade mot någon publik SIP-leverantör.</para>

<para>If you know the URI address of the party that you wish to call, you may choose the Chat -&gt; Call a number action, enter that URI into the sip: input box at the bottom of the window and press the Connect button; eg: sip:foo@ekiga.net and clicking on the Connect button would call the user at that address.</para>

<para>It is also possible to call contacts using the address book, the call history or the roster. You can add contacts you call frequently to your roster, and watch their presence information in order to know when they are available. Please refer to the appropriate section of the manual for full explanations.</para>

<tip><title>Tips</title><para><application>Ekiga</application> har också stöd för H.323 och kan därför ringa till valfri H.323-programvara eller hårdvara. Referera till avsnittet som relaterar till URI:er för att lära dig mer om de olika typerna av URI:er som kan användas för att ringa till fjärranvändare med H.323 och SIP.</para></tip>
</section>

<section><title>Från dator till riktiga telefoner (PC-To-Phone)</title>
<para><application>Ekiga</application> can be used with several Internet Telephony Service Providers. Those providers will allow calling real phones from your computer using <application>Ekiga</application> at interesting rates. We recommend you use the default <application>Ekiga</application> provider. You can get an account using the links in the configuration assistant as described above.</para>

<para>With the default setup, you can simply use sip:3210444555 and select sip.diamondcard.us in the list to call the real phone number +3210444555, 32 being the country code and 10444555 being the number you wish to call.</para>

<para>You can also dial real phone numbers from the address book. If the phone number of the contact you want to call is stored in the address book, simply select Action -&gt; Call [Ekiga Call Out] when the contact is highlighted. It will dial the phone number of the contact using the Ekiga Call Out account.</para>

<tip><title>Tips</title><para><application>Ekiga</application> also supports connecting to H.323 and SIP PBX systems. If the PBX at your office supports those protocols, you will be able to call real phones and be called from real phones after having connected to the PBX. Please ask for the settings from your administrator.</para></tip>
</section>

<section><title>Från riktig telefon till dator (Phone-To-PC)</title>
<para><application>Ekiga</application> kan användas för att ta emot inkommande samtal från vanliga telefoner. För att tillåta det här, kan du helt enkelt logga in med ditt PC-To-Phone-konto via Verktyg-menyn som beskrivs ovanför, och köpa ett telefonnummer i önskat land. <application>Ekiga</application> kommer att ta emot samtalet när folk ringer till det telefonnumret.</para>

<tip><title>Tips</title><para>Du kan faktiskt använda valfri leverantör av H.323 eller SIP-tjänster, inklusive din egna telefonväxel på jobbet. Dock rekommenderar vi att du använder den integrerade leverantören.</para></tip>
</section>

</section>


<section id="ekiga-manage-contacts">
<title>Hantera kontakter</title>

<section><title>Lägg till kontakter till kontaktlistan</title>
<graphic fileref="figures/roster.png"/>

<para>
<application>Ekiga</application> allows you to add the contacts you
dial the most to the roster, so that you can call or start a chat conversation with your friends without having to remember their URI. If supported by the service you are connecting to, <application>Ekiga</application> will display <emphasis>extended presence information</emphasis> about your friends.
Ekiga.net supports publishing presence information for its users. Software PBX systems like <ulink url="http://www.asterisk.org" type="http">Asterisk</ulink> can report if a user is on the phone or not, and <application>Ekiga</application> will display that information in its roster.
</para>

<para>Du kan använda <application>Ekiga</application> för att övervaka linjerna för din telefonväxel.</para>

<para>
<application>Ekiga</application> is also able to detect other <application>Ekiga</application> users on the LAN using the Bonjour technology popularized by Apple (tm) and to display them in the roster. That supposes you have a local mDNSResponder daemon running on your computer. On Linux systems this service will usually be provided by Avahi.
</para>

<para>
To add a contact to the roster, select Chat -&gt; Add Contact, and fill in the required fields. If the service managing the URI you entered for the contact is able to publish presence status, Ekiga will automatically display it.
</para>

<para>
If you do not know the VoIP URI of a contact, you might try searching for him/her using the Ekiga.net online directory. To do so, select Chat -&gt; Address Book, and start searching using the 'Search Filter' feature.
</para>

<tip><title>Tips</title><para>Du kan organisera dina kontakter i grupper i kontaktlistan.</para></tip>
</section>

<section><title>Hantera kontakter</title>
<graphic fileref="figures/addressbook_d1.png"/>

<para>
<application>Ekiga</application> allows you to look for contacts using various sources like the <ulink url="https://www.suse.com/products/desktop/features/evolution.html" type="http">Novell Evolution Email and Calendaring</ulink> address book, any LDAP directory or the Ekiga.net contact directory. You can use the result of your search to start a chat, call the contact, or simply add him to your roster if you have frequent calls with him. To start looking for contacts, select Chat -&gt; Address Book in the menu.
To your left there will be a list dialog showing the LDAP directories as well as a list of local Address Books. The defaults are the <application>Ekiga</application> white pages, and the personal address book from <ulink url="https://www.suse.com/products/desktop/features/evolution.html" type="http">Novell Evolution</ulink>. Support for more contact sources is possible.
</para>

<para>
<application>Ekiga</application> is able to browse any LDAP directory and use any attribute as the calling URI. For example, you could have an LDAP directory in your company, with a specific attribute containing the local extensions of all your colleagues. <application>Ekiga</application> is able to use such an LDAP directory. Simply select in Address Book -&gt; Add an LDAP Address Book, and fill in the required details. You can then right-click on the contact and call him using the call attribute as VoIP URI.
</para>

<graphic fileref="figures/addressbook_d2.png"/>

<para>
The LDAP Address Book supports a range of settings to allow it to work with any LDAPv3 directory. It allows you to choose the attribute to use for displaying a contact's name in the address book as well as a list of attributes for calling info. E.g., if the directory uses the LDAP inetOrgPerson schema you can configure the Address Book to retrieve the homePhone, mobile, and pager attributes make those values available for calling or messaging. You can also customize a Filter Template for the default LDAP search filter, and override the default filter at any time if you need to perform a more specialized search. The browser also supports all security options for LDAP including ldaps:// (LDAP over SSL), StartTLS, and SASL authentication.
</para>

<para>
To refresh the list of users for a specific address book, simply click the Find button. It will search for all users in that address book. You can contact people by double clicking on their highlighted field. You can also message them by right-clicking or by choosing the appropriate action in the Action menu of the window.
</para>

<para>
In certain cases you will want to search specifically for a person name, or his or her call URI in the <application>Ekiga</application> white pages. The address book window allows you to apply filters when searching for contacts. When searching an LDAP directory, entering a simple name in the Search Filter field will perform an LDAP Substring search using the configured Filter Template. If you need to perform a more specialized search you can enter a complete LDAP Filter string, and it will be used instead of the configured Filter Template.
</para>

<tip><title>Tips</title><para>The <application>Ekiga</application> white pages return a limited number of results corresponding to your search. You can then add them to your personal roster to call them later.</para></tip>
</section>

<section><title>Redigera kontakter</title>
<graphic fileref="figures/addressbook_d3.png"/>

<para>
Local address books provided by Novell Evolution allow you to add new contacts, or to edit existing contacts. Each different address book allows a different set of features depending on what makes sense for that specific address book. To discover what features are possible, simply select the address book and consult the Action menu, or right-click on the address book name.
</para>

<para>
To add a contact to one of your local address books, simply select the address book you wish to add the contact to and select Action -&gt; New Contact. The option of adding a New Contact will appear and you may now enter his name and VoIP URI as well as other settings. When finished, select 'OK' and your contact has been added. You can only add contacts to local address books. The contact parameters can be changed at any time by selecting Action -&gt; Edit when the contact is highlighted. He can also be deleted by selecting Action -&gt; Remove.
</para>

<para>
You can also add a contact from the white pages (or any other local or remote address book) to the roster by selecting Action -&gt; Add to local roster.
</para>

</section>

</section>

<section id="ekiga-sending-instant-messages">
<title>Skicka snabbmeddelanden</title>

<graphic fileref="figures/chat_d1.png"/>

<para>
<application>Ekiga</application> allows you to send instant messages to remote users provided that you know their URI.
</para>

<para>
You can send instant messages from the roster, from the call history or from the address book. From the roster or from the call history, simply select Chat -&gt; Contact -&gt; Message in the main window when a contact is highlighted. From the address book window, simply select Action -&gt; Message when the contact is highlighted. A window pops up, enter your text message, and hit the Enter key.
</para>

<tip><title>Tips</title><para>You can not exchange text messages with all protocols. <application>Ekiga</application> will only display the Message menu item when the protocol associated with the user permits it.</para></tip>
</section>


<section id="ekiga-changing-status">
<title>Uppdatera din status</title>

<graphic fileref="figures/status.png"/>

<para>
<application>Ekiga</application> allows you to publish your status to other users.
</para>

<para>
There are three categories of status messages : online, away and busy. Each of them allows you to specify a more complete status information. Simply select Custom message in the status menu at the bottom of the main window. You can then define your extended status message that will be published using all available protocols supporting it.
</para>

<tip><title>Tips</title><para>Many servers will not support relaying your extended presence information. To make sure that this feature is available with the server you are using or with the PBX you are connected to, please ask your administrator. Please note that Ekiga.net will publish your presence information.</para></tip>
</section>


<section id="ekiga-manage-calls">
<title>Hantera samtal</title>

<section><title>Vidarekoppla inkommande samtal</title>
<para>
<application>Ekiga</application> supports different policies for unanswered incoming calls. Per default it displays a popup window which allows you to decide whether you want to refuse or accept the request for an incoming call. If you do not answer the call in the required time, or if you are busy, or if you do not want to receive any call, <application>Ekiga</application> can forward the call to another party.
</para>

<para>
Notice that you need to specify an URI where to forward calls in the preferences to be able to activate that option. Open the preferences window by choosing Edit -&gt; Preferences in the main window and select Call Options on the left. You will now see the appropriate section. It contains three checkboxes for the three cases described above. The URI of the party the calls shall be forwarded to can be configured separately in SIP Settings for SIP and accordingly in H.323 Settings for H.323.
</para>
</section>

<section><title>Kontrollera samtalet</title>
<para><application>Ekiga</application> supports several actions which can be performed when being in a call. These actions enable you to control active sessions. It can be done using the menu and toolbar icons from the call window that appears as soon as a call is setup.</para>

<graphic fileref="figures/call_window.png"/>

<itemizedlist>
<listitem>
<para>Ending a call: The communication to the remote user can be ended by selecting Call -&gt; Hang up.</para>
</listitem>

<listitem>
<para>Holding a call: You can hold a remote party call by selecting Call -&gt; Hold Call. This effectively pauses Video and Audio transmission; to continue transmission again you select Call -&gt; Retrieve Call and Video and Audio Transmission will begin again.</para>
</listitem>

<listitem>
<para>Suspending Audio: This effectively prevents all Audio communication to your respective party when selecting Call -&gt; Mute Audio.</para>
</listitem>

<listitem>
<para>Suspending Video: This effectively prevents all Video transmission to your respective party when selecting Call -&gt; Suspend Video.</para>
</listitem>

<listitem>
<para>Transferring the remote party: You can transfer the remote user to another user by selecting Call -&gt; Transfer Call. It is also possible to transfer an active call by right-clicking and choosing the transfer action when a contact is highlighted in the roster, in the address book or in the call history. Double-clicking or selecting the Contact menu in the main window or the Action menu in the Address Book window and choosing the transfer action will also work.</para>
</listitem>
</itemizedlist>

<tip><title>Tips</title><para>All URIs supported by <application>Ekiga</application> can be used for call transfer if the protocol supports it.</para></tip>
</section>

<section><title>Justera ljud- och videoinställningar</title>
<para>
Your audio and video settings can be adjusted through the call window while you are in a call. The audio volume, but also the brightness, whiteness, color and contrast of your video input device can be changed to achieve the best quality.
</para>

<para>
You can also change your audio and video devices during a call. Simply go in the preferences window by selecting Edit -&gt; Preferences in the menu, and adjust your devices in the appropriate section.
</para>
</section>

<section><title>Kontrollera samtalshistoriken</title>

<graphic fileref="figures/call_history.png"/>

<para>The Call History stores information (date, duration, URI, Remote user) about all outgoing and incoming calls. They are divided into three groups - received calls, placed calls and missed calls. You can consult the call history by selecting View -&gt; Call History in the menu or by clicking on the appropriate icon in the toolbar.</para>

<tip><title>Tips</title><para>Double-clicking on a row in the Calls History will call back the selected user or transfer any active call to that user. Notice that you can also add the contact to your roster by selecting Chat -&gt; Contact -&gt; Add to local roster in the main menu when the call is highlighted.</para></tip>
</section>

</section>
</section>

<section id="ekiga-advanced-usage">
<title>Avancerad användning</title>

<section id="ekiga-registering-additional-accounts">
<title>Registrera ytterligare konton</title>

<section><title>Kontofönstret</title>

<graphic fileref="figures/accounts_d1.png"/>

<para>
You can open the accounts window by selecting Edit -&gt; Accounts. This will open the accounts window. The accounts window will allow you to add Ekiga.net, Ekiga Call Out, SIP and H.323 accounts and to register to them.
An account describes the user login and password parameters to register to SIP and H.323 services. Those <emphasis>services</emphasis> can be an Internet Telephony Service provider (like ekiga.net), or an IPBX (like CISCO, Nortel, or Asterisk).
</para>
</section>

<section><title>Lägg till ett Ekiga-konto</title>

<graphic fileref="figures/accounts_ekiga_net.png"/>

<para>
To add an Ekiga.net account, simply select Accounts -&gt; Add an Ekiga.net Account in the menu. A dialog will appear and allow you to enter several parameters:
<itemizedlist>
<listitem><para><emphasis>Användare:</emphasis> Du kan ange ditt inloggningsnamn.</para></listitem>
<listitem><para><emphasis>Lösenord:</emphasis> Du kan ange ditt lösenord.</para></listitem>
</itemizedlist>
</para>

<para>
Ekiga.net is a free SIP services platform provided to <application>Ekiga</application> users.
If you want to call other users and to be callable, you need a SIP address. You can get one from <ulink url="http://www.ekiga.net" type="http">http://www.ekiga.net</ulink>.
Ekiga.net also offers additional services like conference rooms, voice mail and online white pages. Please see <ulink url="http://www.ekiga.net" type="http">http://www.ekiga.net</ulink> for more information.
</para>
</section>

<section><title>Lägg till ett Ekiga Ring ut-konto</title>

<graphic fileref="figures/accounts_ekiga_call_out.png"/>

<para>
To add an Ekiga Call Out account, simply select Accounts -&gt; Add an Ekiga Call Out Account in the menu. A dialog will appear and allow you to enter several parameters:
<itemizedlist>
<listitem><para><emphasis>Konto-ID:</emphasis> Du kan ange ditt konto-id.</para></listitem>
<listitem><para><emphasis>PIN-kod:</emphasis> Du kan ange din PIN-kod.</para></listitem>
</itemizedlist>
</para>

<para>
If you do not have an Ekiga Call Out account yet, you can subscribe for one using the 'Get an Ekiga.net Call Out account' link in the dialog.
As described above, this service will allow you to call normal phones worldwide at interesting rates.
Once the account has been added, you can recharge it, consult the balance history or the call history by selecting the appropriate menu item in the Account menu of the window when the account is highlighted.
</para>
</section>

<section><title>Lägg till ett SIP-konto</title>

<graphic fileref="figures/accounts_sip.png"/>

<para>
To add a SIP account, simply select Accounts -&gt; Add a SIP Account in the menu. A dialog will appear and allow you to enter several parameters:
<itemizedlist>
<listitem><para><emphasis>Namn:</emphasis> Du kan ange kontonamnet.</para></listitem>
<listitem><para><emphasis>Registrator:</emphasis> Registratorn till vilken du vill registrera dig. Det här är vanligtvis en IP-adress eller ett värdnamn som ges till dig av din IP-telefonileverantör, eller av din administratör om du försöker registrera dig mot en Internet-ansluten SIP-telefonväxel.</para></listitem>
<listitem><para><emphasis>Användare:</emphasis> Du kan ange ditt inloggningsnamn.</para></listitem>
<listitem><para><emphasis>Användarnamn för autentisering:</emphasis> Om det är annorlunda för användarparametern som du angav ovan. I det fallet kommer användarfältet att användas för att kontrollera den utgående identiteten för kontot som du lägger till, och inloggningsnamnet kommer att användas under autentiseringsfasen.</para></listitem>
<listitem><para><emphasis>Lösenord:</emphasis> Du kan ange ditt lösenord.</para></listitem>
<listitem><para><emphasis>Tidsgräns:</emphasis> Tidsgränsen efter vilken registreringen ska uppdateras.</para></listitem>
</itemizedlist>
</para>

</section>

<section><title>Lägg till ett H.323-konto</title>

<graphic fileref="figures/accounts_h323.png"/>

<para>
To add an H.323 account, simply select Accounts -&gt; Add an H.323 Account in the menu. A dialog will appear and allow you to enter several parameters:
<itemizedlist>
<listitem><para><emphasis>Namn:</emphasis> Du kan ange kontonamnet.</para></listitem>
<listitem><para><emphasis>Gatekeeper:</emphasis> The gatekeeper to which you want to register. This is usually an IP address or a host name that will be given to you by your Internet Telephony Service Provider, or by your administrator if you are trying to register to an H.323 IPBX.</para></listitem>
<listitem><para><emphasis>Användare:</emphasis> Du kan ange ditt inloggningsnamn.</para></listitem>
<listitem><para><emphasis>Användarnamn för autentisering:</emphasis> Om det är annorlunda för användarparametern som du angav ovan. I det fallet kommer användarfältet att användas för att kontrollera den utgående identiteten för kontot som du lägger till, och inloggningsnamnet kommer att användas under autentiseringsfasen.</para></listitem>
<listitem><para><emphasis>Lösenord:</emphasis> Du kan ange ditt lösenord.</para></listitem>
<listitem><para><emphasis>Tidsgräns för registrering:</emphasis> Tidsgränsen efter vilken registreringen ska uppdateras.</para></listitem>
</itemizedlist>
</para>

</section>

</section>

<section id="ekiga-uris">
<title>Förstå URI:er</title>

<section><title>SIP URI:er</title>

<para>SIP URI:er är formaterade som "sip:användare@[värd[:port]]"</para>

<para>Det här låter dig ringa upp angiven användare eller anknytning på angiven SIP-proxy: <emphasis>sip:jonita@ekiga.net</emphasis></para>
</section>


<section><title>H.323 URI:er</title>

<para>H.323 URI:er är formaterade som "h323:[användare@][värd[:port]]"</para>

<para>Det här låter dig att: <itemizedlist>
<listitem><para>Ring upp angiven värd på en annan port istället för standardporten, vilken är 1720: <emphasis>h323:seconix.com:1740</emphasis></para></listitem>
<listitem><para>Ring upp en angiven användare med dennes respektive alias om registrerad mot en portvakt: <emphasis>h323:jonita</emphasis></para></listitem>
<listitem><para>Ring upp angivet telefonnummer om du är registrerad mot en portvakt för en PC-To-Phone-leverantör, eller om den användaren har ett ENUM-objekt associerat till en H.323-URI: <emphasis>h323:003210111222</emphasis></para></listitem>
<listitem><para>Ring upp en angiven användare med dennes alias genom en specifik gateway eller proxy: <emphasis>h323:jonita@gateway.seconix.com</emphasis></para></listitem>
<listitem><para>Ring upp en MCU och gå in i ett specifikt rum: <emphasis>h323:minvänsrum@mcu.seconix.com</emphasis></para></listitem>
</itemizedlist></para>
</section>

</section>


<section id="ekiga-video-bandwidth">
<title>Kontrollera videobandbredden</title>

<para><application>Ekiga</application> uses a best-effort algorithm to maintain a low bandwidth when transmitting video.  It will permit <application>Ekiga</application> to dynamically adjust the video bandwidth and the number of transmitted images per second during a call while trying to respect the requested video bandwidth.</para>

<para>Notice that the algorithm is a best-effort algorithm, which means that if your video bandwidth settings are too low, it can be impossible to respect them. However, if the video bandwidth permits to transmit with a better quality, or faster than the requested values, then <application>Ekiga</application> will dynamically increase them so that the quality and the framerate are always the best possible.</para>

<!-- <para>Choosing a higher framerate and a lower quality will have the same result in terms of video bandwidth as choosing a higher quality with a lower framerate. The choice depends on if you prefer using your bandwidth to transmit more lower quality images or fewer high quality images.</para>-->
</section>


<section id="ekiga-monitoring-lines">
<title>Övervaka linjer</title>

<graphic fileref="figures/monitoring_lines.png"/>

<para><application>Ekiga</application> kan ansluta till telefonväxelsystem som har stöds för SIP-protokollet. I det fallet kan det indikera om en linje som är associerad med en användare används eller inte. Referera till dokumentationen för din telefonväxel för att aktivera funktionen.</para>

<para>To enable that feature on <application>Ekiga</application>, simply add the contact with his URI in the roster. If the server supports publishing presence information, <application>Ekiga</application> will automatically publish your own presence information and display the presence of contacts in your roster.</para>
</section>

<section id="ekiga-audio-codecs">
<title>Hantera kodekar</title>

<section><title>Ljudkodekar</title>

<graphic fileref="figures/audio_codecs.png"/>

<para>
The <application>Ekiga</application> audio codecs table in the preferences permits you to change the codec order as well as disabling the codecs you don't want to use. Each codec has strong and weak points. For example, G.711 will give the best voice quality but will use the most bandwidth while SPEEX will give an average voice quality but requiring a very low bandwidth usage. Notice that there are two versions of SPEEX; one of them is SPEEX WideBand, which has a 16 kHz clock rate.</para>
</section>

<section><title>Videokodekar</title>

<graphic fileref="figures/video_codecs.png"/>

<para>
The <application>Ekiga</application> video codecs table in the preferences permits you to change the codec order as well as disabling the codecs you don't want to use. <application>Ekiga</application> supports codecs like H.261, H.263+, H.264, MPEG-4 or Theora.</para>
</section>


<section><title>Ändra ordning på kodekar</title>
<para>
When you reorder the codecs, you are reordering the local capabilities table, ie the codecs you will use for sending. The codec used is the first active codec on receiver which is active on sender.</para>
</section>

<section><title>Tvinga användningen av en specifik kodek</title>
<para>
You can force the use of a specific codec by disabling all other codecs, but it will result in failed calls if the remote user doesn't support that specific codec. The best approach is to put your preferred codecs at the top of the list so that you always transmit with them if the remote user allows it and to disable the codecs that you don't want to use for transmission and reception.</para>
</section>

<section><title>Justera jitterbufferten</title>
<para>
You can adjust the delay to wait before playing the sound buffers that you have received using the jitter buffer adjustment. If there is too much packet loss, the delay required to have received all packets could be so important that it will exceed the jitter buffer. In such a case, the sound you are receiving will be of bad quality. A solution to that problem would be to increase the maximum limit of the jitter buffer to a few seconds, resulting in a big delay but in an improved voice quality. Notice that the jitter buffer will readapt itself to the lowest delay allowing for optimum transmission, and that a bad voice quality in reception is not due to a too low jitter buffer value, but to bad internet connection quality.
</para>
</section>

</section>


<section id="ekiga-defining-ports">
<title>Ändra portar</title>

<section><title>Lyssningsportarna</title>
<para>
The main port used to listen for incoming connections in <application>Ekiga</application> for SIP is port 5060 (UDP), while 1720 (TCP) is used by H.323. To change those ports you need to load "gconf-editor". Open gconf-editor, select apps from the left hand side menu and then select <application>Ekiga</application>, Protocols. Then select "sip" or "h323", it should give you a list in the corresponding window to your right. Select listen_port and change it to your desired value. You can also change the UDP/RTP port ranges.
</para>
</section>

<section><title>Förklaring av portintervallen</title>

<para>1. The "listen_port" value is the port <application>Ekiga</application> will use to listen for incoming connections. It is different for SIP and H.323.</para>

<para>2. The "udp_port_range" value is the range of UDP ports that <application>Ekiga</application> will use for SIP signalling or when registering to H.323 gatekeepers. It is also used for RTP (audio and video communication channels).</para>

<para>3. The "tcp_port_range" value is the range of TCP ports beside the listen_port that <application>Ekiga</application> will use for the H.245 channel with the H.323 protocol. That port range is not used by SIP. It is also not used when H.245 Tunneling is enabled, which is generally the case, except when calling old H.323 implementations like Netmeeting.</para>
</section>
</section>


<section id="controlling-sip-h323-settings">
<title>Kontrollera SIP- och H.323-inställningarna</title>
<section id="ekiga-sip">
<title>Kontrollera SIP-inställningarna</title>

<section><title>Diverse inställningar</title>
<para><emphasis>Utgående proxy</emphasis></para>
<para>The outbound proxy is the SIP proxy that will relay your calls. The behavior of a SIP proxy is similar to the behavior of an HTTP proxy, i.e. some entity that issues the requests on your behalf and proxies the streams.</para>

<para><emphasis>Vidarekopplings-URI</emphasis></para>
<para>URI:en till vilken inkommande SIP-samtal ska vidarekopplas till om det är konfigurerat i inställningarna.</para>

</section>
</section>

<section id="ekiga-h323">
<title>Kontrollera H.323-inställningarna</title>

<section><title>Diverse inställningar</title>
<para><emphasis>Vidarekopplings-URI</emphasis></para>
<para>URI:en till vilken inkommande H.323-samtal ska vidarekopplas till om det konfigurerats i inställningarna.</para>

</section>

<section><title>Avancerade inställningar</title>
<para><application>Ekiga</application> tillåter en bra kontroll över H.323-inställningarna i sektionen Avancerade H.323-inställningar i inställningarna. Du kan aktivera H.245-tunnling, Tidig H.245 och Snabbstart.</para>

<para><emphasis>H.245-tunnling</emphasis></para>

<para>H.245-tunnling är inkapsling av H.245-meddelanden i H.225/Q.931-meddelanden (H.245-tunnling). Om u har en brandvägg och aktiverar H.245-tunnling, är det en mindre TCP-port som du behöver tillåta för inkommande anslutningar.</para>

<para><emphasis>Tidig H.245</emphasis></para>

<para>Det här aktiverar H.245 tidigt i uppsättningen och gör att initiering av samtal går fortare.</para>

<para><emphasis>Snabbstart</emphasis></para>

<para>Snabbstart är en ny metod för att ringa ett samtal som går förbi vissa vanliga steg för att det ska gå snabbare. I tillägg till hastighetsökningen tillåter Snabbstart att mediakanalerna blir operationella innan CONNECT-meddelandet skickas, vilket är ett krav för vissa betalningssätt. Det introducerades i H.323 version 2. </para>
</section>

</section>
</section>
</section>

<section id="ekiga-about">
<title>Om <application>Ekiga</application></title>
<para><application>Ekiga</application> is written by Damien Sandras (<email>dsandras@seconix.com</email>) with the help of many volunteers. Active maintainers are Damien Sandras (<email>dsandras@seconix.com</email>), Eugen Dedu (<email>Eugen.Dedu@pu-pm.univ-fcomte.fr</email>) and Julien Puydt (<email>jpuydt@free.fr</email>).
To find more information about <application>Ekiga</application>, please visit the <ulink url="http://www.ekiga.org" type="http"><application>Ekiga</application> Home Page</ulink>.
</para>

<para>För att rapportera ett fel eller skicka in förslag angående det här programmet eller den här handboken, följ anvisningarna i det här <ulink url="ghelp:user-guide?feedback" type="help">dokumentet</ulink>.</para>

<para>Detta program distribueras under villkoren i GNU General Public License, publicerad av Free Software Foundation, antingen version 2 av licensen, eller (om du så vill) någon senare version. En kopia av den här licensen kan hittas på den här <ulink url="ghelp:gpl" type="help">länken</ulink>, eller i filen COPYING som inkluderats i källkoden för det här programmet.</para>
</section>



<section id="ekiga-appendix">
<title>Appendix</title>

<section id="ekiga-related">
<title>Relaterad programvara</title>

<para><emphasis>IPBX</emphasis></para>
<itemizedlist>
<listitem><para>Asterisk PBX: <ulink url="http://asterisk.org" type="http">http://asterisk.org</ulink></para></listitem>
</itemizedlist>

<para><emphasis>SIP</emphasis></para>
<itemizedlist>
<listitem><para>SIP Express Router: <ulink url="http://www.iptel.org/ser" type="http">http://www.iptel.org/ser</ulink></para></listitem>
</itemizedlist>

<para><emphasis>H.323</emphasis></para>
<itemizedlist>
<listitem><para>OpenH323 Gatekeeper: <ulink url="http://www.openh323.org" type="http">http://www.openh323.org</ulink></para></listitem>
<listitem><para>GNU Gatekeeper: <ulink url="http://www.gnugk.org" type="http">http://www.gnugk.org</ulink></para></listitem>
<listitem><para>OpenH323 Proxy: <ulink url="http://openh323.sourceforge.net" type="http">http://openh323.sourceforge.net</ulink></para></listitem>
<listitem><para>H323 - ISDN Gateway: <ulink url="http://www.telos.de/linux/H323/" type="http">http://www.telos.de/linux/H323/</ulink></para></listitem>
</itemizedlist>

<para><emphasis>Konferens/VoIP-programvara</emphasis></para>

<itemizedlist>
<listitem><para>OpenMCU: <ulink url="http://www.openh323.org" type="http">http://www.openh323.org</ulink></para></listitem>
</itemizedlist>

<para><emphasis>Liknande klienter</emphasis></para>

<itemizedlist>
<listitem><para>XTen: <ulink url="http://www.xten.com" type="http">http://www.xten.com</ulink></para></listitem>
<listitem><para>SJPhone: <ulink url="http://www.sjlabs.com/" type="http">http://www.sjlabs.com/</ulink></para></listitem>
<listitem><para>OpenPhone: <ulink url="http://www.openh323.org" type="http">http://www.openh323.org</ulink></para></listitem>
<listitem><para>Netmeeting: <ulink url="http://www.microsoft.com" type="http">http://www.microsoft.com</ulink></para></listitem>
</itemizedlist>

</section>
</section>

</article>
<!-- END -->
