<?xml version="1.0"?>
<!DOCTYPE lmms-project>
<lmms-project type="song" version="1.0" creator="LMMS" creatorversion="1.2.0">
  <head timesig_denominator="4" bpm="140" masterpitch="0" mastervol="100" timesig_numerator="4"/>
  <song>
    <trackcontainer visible="1" width="600" height="300" type="song" x="6" y="5" maximized="0" minimized="0">
      <track type="0" muted="0" name="Default" solo="0">
        <instrumenttrack pitch="0" vol="100" fxch="0" pan="0" basenote="57" usemasterpitch="1" pitchrange="1">
          <instrument name="tripleoscillator">
            <tripleoscillator finel0="0" vol1="33" finel1="0" coarse0="0" finer0="0" vol2="33" pan0="0" finer1="0" coarse1="0" finel2="0" pan1="0" coarse2="0" finer2="0" pan2="0" wavetype0="0" wavetype1="0" wavetype2="0" phoffset0="0" phoffset1="0" phoffset2="0" modalgo1="2" modalgo2="2" modalgo3="2" stphdetun0="0" stphdetun1="0" stphdetun2="0" userwavefile0="" userwavefile1="" userwavefile2="" vol0="33"/>
          </instrument>
          <eldata fwet="0" ftype="0" fres="0.5" fcut="14000">
            <elvol lspd="0.1" ctlenvamt="0" lpdel="0" pdel="0" amt="0" hold="0.5" syncmode="0" userwavefile="" latt="0" sustain="0.5" lamt="0" lshp="0" lspd_denominator="4" lspd_numerator="4" x100="0" rel="0.1" dec="0.5" att="0"/>
            <elcut lspd="0.1" ctlenvamt="0" lpdel="0" pdel="0" amt="0" hold="0.5" syncmode="0" userwavefile="" latt="0" sustain="0.5" lamt="0" lshp="0" lspd_denominator="4" lspd_numerator="4" x100="0" rel="0.1" dec="0.5" att="0"/>
            <elres lspd="0.1" ctlenvamt="0" lpdel="0" pdel="0" amt="0" hold="0.5" syncmode="0" userwavefile="" latt="0" sustain="0.5" lamt="0" lshp="0" lspd_denominator="4" lspd_numerator="4" x100="0" rel="0.1" dec="0.5" att="0"/>
          </eldata>
          <chordcreator chordrange="1" chord="0" chord-enabled="0"/>
          <arpeggiator arpdir="0" arpgate="100" arptime_denominator="4" syncmode="0" arp-enabled="0" arprange="1" arptime_numerator="4" arpmode="0" arp="0" arptime="100"/>
          <midiport inputchannel="0" fixedinputvelocity="-1" outputcontroller="0" outputchannel="1" fixedoutputvelocity="-1" readable="0" fixedoutputnote="-1" outputprogram="1" writable="0" basevelocity="127" inputcontroller="0"/>
          <fxchain numofeffects="0" enabled="0"/>
        </instrumenttrack>
      </track>
      <track type="1" muted="0" name="Beat/Bassline 0" solo="0">
        <bbtrack>
          <trackcontainer visible="1" width="580" height="300" type="bbtrackcontainer" x="610" y="5" maximized="0" minimized="0">
            <track type="0" muted="0" name="Clap.ds" solo="0">
              <instrumenttrack pitch="0" vol="100" fxch="1" pan="0" basenote="57" usemasterpitch="1" pitchrange="1">
                <instrument name="audiofileprocessor">
                  <audiofileprocessor interp="1" reversed="0" looped="0" sframe="0" lframe="0" eframe="1" src="drumsynth/cr8000/Clap.ds" amp="100" stutter="0"/>
                </instrument>
                <eldata fwet="0" ftype="0" fres="0.5" fcut="14000">
                  <elvol lspd="0.1" ctlenvamt="0" lpdel="0" pdel="0" amt="0" hold="0.5" syncmode="0" userwavefile="" latt="0" sustain="0.5" lamt="0" lshp="0" lspd_denominator="4" lspd_numerator="4" x100="0" rel="0.1" dec="0.5" att="0"/>
                  <elcut lspd="0.1" ctlenvamt="0" lpdel="0" pdel="0" amt="0" hold="0.5" syncmode="0" userwavefile="" latt="0" sustain="0.5" lamt="0" lshp="0" lspd_denominator="4" lspd_numerator="4" x100="0" rel="0.1" dec="0.5" att="0"/>
                  <elres lspd="0.1" ctlenvamt="0" lpdel="0" pdel="0" amt="0" hold="0.5" syncmode="0" userwavefile="" latt="0" sustain="0.5" lamt="0" lshp="0" lspd_denominator="4" lspd_numerator="4" x100="0" rel="0.1" dec="0.5" att="0"/>
                </eldata>
                <chordcreator chordrange="1" chord="0" chord-enabled="0"/>
                <arpeggiator arpdir="0" arpgate="100" arptime_denominator="4" syncmode="0" arp-enabled="0" arprange="1" arptime_numerator="4" arpmode="0" arp="0" arptime="100"/>
                <midiport inputchannel="0" fixedinputvelocity="-1" outputcontroller="0" outputchannel="1" fixedoutputvelocity="-1" readable="0" fixedoutputnote="-1" outputprogram="1" writable="0" basevelocity="127" inputcontroller="0"/>
                <fxchain numofeffects="0" enabled="0"/>
              </instrumenttrack>
              <pattern type="0" muted="0" steps="16" name="Clap.ds" pos="0" len="192"/>
            </track>
            <track type="0" muted="0" name="Clave.ds" solo="0">
              <instrumenttrack pitch="0" vol="100" fxch="1" pan="0" basenote="57" usemasterpitch="1" pitchrange="1">
                <instrument name="audiofileprocessor">
                  <audiofileprocessor interp="1" reversed="0" looped="0" sframe="0" lframe="0" eframe="1" src="drumsynth/cr8000/Clave.ds" amp="100" stutter="0"/>
                </instrument>
                <eldata fwet="0" ftype="0" fres="0.5" fcut="14000">
                  <elvol lspd="0.1" ctlenvamt="0" lpdel="0" pdel="0" amt="0" hold="0.5" syncmode="0" userwavefile="" latt="0" sustain="0.5" lamt="0" lshp="0" lspd_denominator="4" lspd_numerator="4" x100="0" rel="0.1" dec="0.5" att="0"/>
                  <elcut lspd="0.1" ctlenvamt="0" lpdel="0" pdel="0" amt="0" hold="0.5" syncmode="0" userwavefile="" latt="0" sustain="0.5" lamt="0" lshp="0" lspd_denominator="4" lspd_numerator="4" x100="0" rel="0.1" dec="0.5" att="0"/>
                  <elres lspd="0.1" ctlenvamt="0" lpdel="0" pdel="0" amt="0" hold="0.5" syncmode="0" userwavefile="" latt="0" sustain="0.5" lamt="0" lshp="0" lspd_denominator="4" lspd_numerator="4" x100="0" rel="0.1" dec="0.5" att="0"/>
                </eldata>
                <chordcreator chordrange="1" chord="0" chord-enabled="0"/>
                <arpeggiator arpdir="0" arpgate="100" arptime_denominator="4" syncmode="0" arp-enabled="0" arprange="1" arptime_numerator="4" arpmode="0" arp="0" arptime="100"/>
                <midiport inputchannel="0" fixedinputvelocity="-1" outputcontroller="0" outputchannel="1" fixedoutputvelocity="-1" readable="0" fixedoutputnote="-1" outputprogram="1" writable="0" basevelocity="127" inputcontroller="0"/>
                <fxchain numofeffects="0" enabled="0"/>
              </instrumenttrack>
              <pattern type="0" muted="0" steps="16" name="Clave.ds" pos="0" len="192"/>
            </track>
            <track type="0" muted="0" name="Conga_l.ds" solo="0">
              <instrumenttrack pitch="0" vol="100" fxch="1" pan="0" basenote="57" usemasterpitch="1" pitchrange="1">
                <instrument name="audiofileprocessor">
                  <audiofileprocessor interp="1" reversed="0" looped="0" sframe="0" lframe="0" eframe="1" src="drumsynth/cr8000/Conga_l.ds" amp="100" stutter="0"/>
                </instrument>
                <eldata fwet="0" ftype="0" fres="0.5" fcut="14000">
                  <elvol lspd="0.1" ctlenvamt="0" lpdel="0" pdel="0" amt="0" hold="0.5" syncmode="0" userwavefile="" latt="0" sustain="0.5" lamt="0" lshp="0" lspd_denominator="4" lspd_numerator="4" x100="0" rel="0.1" dec="0.5" att="0"/>
                  <elcut lspd="0.1" ctlenvamt="0" lpdel="0" pdel="0" amt="0" hold="0.5" syncmode="0" userwavefile="" latt="0" sustain="0.5" lamt="0" lshp="0" lspd_denominator="4" lspd_numerator="4" x100="0" rel="0.1" dec="0.5" att="0"/>
                  <elres lspd="0.1" ctlenvamt="0" lpdel="0" pdel="0" amt="0" hold="0.5" syncmode="0" userwavefile="" latt="0" sustain="0.5" lamt="0" lshp="0" lspd_denominator="4" lspd_numerator="4" x100="0" rel="0.1" dec="0.5" att="0"/>
                </eldata>
                <chordcreator chordrange="1" chord="0" chord-enabled="0"/>
                <arpeggiator arpdir="0" arpgate="100" arptime_denominator="4" syncmode="0" arp-enabled="0" arprange="1" arptime_numerator="4" arpmode="0" arp="0" arptime="100"/>
                <midiport inputchannel="0" fixedinputvelocity="-1" outputcontroller="0" outputchannel="1" fixedoutputvelocity="-1" readable="0" fixedoutputnote="-1" outputprogram="1" writable="0" basevelocity="127" inputcontroller="0"/>
                <fxchain numofeffects="0" enabled="0"/>
              </instrumenttrack>
              <pattern type="0" muted="0" steps="16" name="Conga_l.ds" pos="0" len="192"/>
            </track>
            <track type="0" muted="0" name="Conga_m.ds" solo="0">
              <instrumenttrack pitch="0" vol="100" fxch="1" pan="0" basenote="57" usemasterpitch="1" pitchrange="1">
                <instrument name="audiofileprocessor">
                  <audiofileprocessor interp="1" reversed="0" looped="0" sframe="0" lframe="0" eframe="1" src="drumsynth/cr8000/Conga_m.ds" amp="100" stutter="0"/>
                </instrument>
                <eldata fwet="0" ftype="0" fres="0.5" fcut="14000">
                  <elvol lspd="0.1" ctlenvamt="0" lpdel="0" pdel="0" amt="0" hold="0.5" syncmode="0" userwavefile="" latt="0" sustain="0.5" lamt="0" lshp="0" lspd_denominator="4" lspd_numerator="4" x100="0" rel="0.1" dec="0.5" att="0"/>
                  <elcut lspd="0.1" ctlenvamt="0" lpdel="0" pdel="0" amt="0" hold="0.5" syncmode="0" userwavefile="" latt="0" sustain="0.5" lamt="0" lshp="0" lspd_denominator="4" lspd_numerator="4" x100="0" rel="0.1" dec="0.5" att="0"/>
                  <elres lspd="0.1" ctlenvamt="0" lpdel="0" pdel="0" amt="0" hold="0.5" syncmode="0" userwavefile="" latt="0" sustain="0.5" lamt="0" lshp="0" lspd_denominator="4" lspd_numerator="4" x100="0" rel="0.1" dec="0.5" att="0"/>
                </eldata>
                <chordcreator chordrange="1" chord="0" chord-enabled="0"/>
                <arpeggiator arpdir="0" arpgate="100" arptime_denominator="4" syncmode="0" arp-enabled="0" arprange="1" arptime_numerator="4" arpmode="0" arp="0" arptime="100"/>
                <midiport inputchannel="0" fixedinputvelocity="-1" outputcontroller="0" outputchannel="1" fixedoutputvelocity="-1" readable="0" fixedoutputnote="-1" outputprogram="1" writable="0" basevelocity="127" inputcontroller="0"/>
                <fxchain numofeffects="0" enabled="0"/>
              </instrumenttrack>
              <pattern type="0" muted="0" steps="16" name="Conga_m.ds" pos="0" len="192"/>
            </track>
            <track type="0" muted="0" name="Cowbell.ds" solo="0">
              <instrumenttrack pitch="0" vol="100" fxch="1" pan="0" basenote="57" usemasterpitch="1" pitchrange="1">
                <instrument name="audiofileprocessor">
                  <audiofileprocessor interp="1" reversed="0" looped="0" sframe="0" lframe="0" eframe="1" src="drumsynth/cr8000/Cowbell.ds" amp="100" stutter="0"/>
                </instrument>
                <eldata fwet="0" ftype="0" fres="0.5" fcut="14000">
                  <elvol lspd="0.1" ctlenvamt="0" lpdel="0" pdel="0" amt="0" hold="0.5" syncmode="0" userwavefile="" latt="0" sustain="0.5" lamt="0" lshp="0" lspd_denominator="4" lspd_numerator="4" x100="0" rel="0.1" dec="0.5" att="0"/>
                  <elcut lspd="0.1" ctlenvamt="0" lpdel="0" pdel="0" amt="0" hold="0.5" syncmode="0" userwavefile="" latt="0" sustain="0.5" lamt="0" lshp="0" lspd_denominator="4" lspd_numerator="4" x100="0" rel="0.1" dec="0.5" att="0"/>
                  <elres lspd="0.1" ctlenvamt="0" lpdel="0" pdel="0" amt="0" hold="0.5" syncmode="0" userwavefile="" latt="0" sustain="0.5" lamt="0" lshp="0" lspd_denominator="4" lspd_numerator="4" x100="0" rel="0.1" dec="0.5" att="0"/>
                </eldata>
                <chordcreator chordrange="1" chord="0" chord-enabled="0"/>
                <arpeggiator arpdir="0" arpgate="100" arptime_denominator="4" syncmode="0" arp-enabled="0" arprange="1" arptime_numerator="4" arpmode="0" arp="0" arptime="100"/>
                <midiport inputchannel="0" fixedinputvelocity="-1" outputcontroller="0" outputchannel="1" fixedoutputvelocity="-1" readable="0" fixedoutputnote="-1" outputprogram="1" writable="0" basevelocity="127" inputcontroller="0"/>
                <fxchain numofeffects="0" enabled="0"/>
              </instrumenttrack>
              <pattern type="0" muted="0" steps="16" name="Cowbell.ds" pos="0" len="192"/>
            </track>
            <track type="0" muted="0" name="Cymbal.ds" solo="0">
              <instrumenttrack pitch="0" vol="100" fxch="1" pan="0" basenote="57" usemasterpitch="1" pitchrange="1">
                <instrument name="audiofileprocessor">
                  <audiofileprocessor interp="1" reversed="0" looped="0" sframe="0" lframe="0" eframe="1" src="drumsynth/cr8000/Cymbal.ds" amp="100" stutter="0"/>
                </instrument>
                <eldata fwet="0" ftype="0" fres="0.5" fcut="14000">
                  <elvol lspd="0.1" ctlenvamt="0" lpdel="0" pdel="0" amt="0" hold="0.5" syncmode="0" userwavefile="" latt="0" sustain="0.5" lamt="0" lshp="0" lspd_denominator="4" lspd_numerator="4" x100="0" rel="0.1" dec="0.5" att="0"/>
                  <elcut lspd="0.1" ctlenvamt="0" lpdel="0" pdel="0" amt="0" hold="0.5" syncmode="0" userwavefile="" latt="0" sustain="0.5" lamt="0" lshp="0" lspd_denominator="4" lspd_numerator="4" x100="0" rel="0.1" dec="0.5" att="0"/>
                  <elres lspd="0.1" ctlenvamt="0" lpdel="0" pdel="0" amt="0" hold="0.5" syncmode="0" userwavefile="" latt="0" sustain="0.5" lamt="0" lshp="0" lspd_denominator="4" lspd_numerator="4" x100="0" rel="0.1" dec="0.5" att="0"/>
                </eldata>
                <chordcreator chordrange="1" chord="0" chord-enabled="0"/>
                <arpeggiator arpdir="0" arpgate="100" arptime_denominator="4" syncmode="0" arp-enabled="0" arprange="1" arptime_numerator="4" arpmode="0" arp="0" arptime="100"/>
                <midiport inputchannel="0" fixedinputvelocity="-1" outputcontroller="0" outputchannel="1" fixedoutputvelocity="-1" readable="0" fixedoutputnote="-1" outputprogram="1" writable="0" basevelocity="127" inputcontroller="0"/>
                <fxchain numofeffects="0" enabled="0"/>
              </instrumenttrack>
              <pattern type="0" muted="0" steps="16" name="Cymbal.ds" pos="0" len="192"/>
            </track>
            <track type="0" muted="0" name="Hat_c.ds" solo="0">
              <instrumenttrack pitch="0" vol="100" fxch="1" pan="0" basenote="57" usemasterpitch="1" pitchrange="1">
                <instrument name="audiofileprocessor">
                  <audiofileprocessor interp="1" reversed="0" looped="0" sframe="0" lframe="0" eframe="1" src="drumsynth/cr8000/Hat_c.ds" amp="100" stutter="0"/>
                </instrument>
                <eldata fwet="0" ftype="0" fres="0.5" fcut="14000">
                  <elvol lspd="0.1" ctlenvamt="0" lpdel="0" pdel="0" amt="0" hold="0.5" syncmode="0" userwavefile="" latt="0" sustain="0.5" lamt="0" lshp="0" lspd_denominator="4" lspd_numerator="4" x100="0" rel="0.1" dec="0.5" att="0"/>
                  <elcut lspd="0.1" ctlenvamt="0" lpdel="0" pdel="0" amt="0" hold="0.5" syncmode="0" userwavefile="" latt="0" sustain="0.5" lamt="0" lshp="0" lspd_denominator="4" lspd_numerator="4" x100="0" rel="0.1" dec="0.5" att="0"/>
                  <elres lspd="0.1" ctlenvamt="0" lpdel="0" pdel="0" amt="0" hold="0.5" syncmode="0" userwavefile="" latt="0" sustain="0.5" lamt="0" lshp="0" lspd_denominator="4" lspd_numerator="4" x100="0" rel="0.1" dec="0.5" att="0"/>
                </eldata>
                <chordcreator chordrange="1" chord="0" chord-enabled="0"/>
                <arpeggiator arpdir="0" arpgate="100" arptime_denominator="4" syncmode="0" arp-enabled="0" arprange="1" arptime_numerator="4" arpmode="0" arp="0" arptime="100"/>
                <midiport inputchannel="0" fixedinputvelocity="-1" outputcontroller="0" outputchannel="1" fixedoutputvelocity="-1" readable="0" fixedoutputnote="-1" outputprogram="1" writable="0" basevelocity="127" inputcontroller="0"/>
                <fxchain numofeffects="0" enabled="0"/>
              </instrumenttrack>
              <pattern type="0" muted="0" steps="16" name="Hat_c.ds" pos="0" len="192"/>
            </track>
            <track type="0" muted="0" name="Hat_o.ds" solo="0">
              <instrumenttrack pitch="0" vol="100" fxch="1" pan="0" basenote="57" usemasterpitch="1" pitchrange="1">
                <instrument name="audiofileprocessor">
                  <audiofileprocessor interp="1" reversed="0" looped="0" sframe="0" lframe="0" eframe="1" src="drumsynth/cr8000/Hat_o.ds" amp="100" stutter="0"/>
                </instrument>
                <eldata fwet="0" ftype="0" fres="0.5" fcut="14000">
                  <elvol lspd="0.1" ctlenvamt="0" lpdel="0" pdel="0" amt="0" hold="0.5" syncmode="0" userwavefile="" latt="0" sustain="0.5" lamt="0" lshp="0" lspd_denominator="4" lspd_numerator="4" x100="0" rel="0.1" dec="0.5" att="0"/>
                  <elcut lspd="0.1" ctlenvamt="0" lpdel="0" pdel="0" amt="0" hold="0.5" syncmode="0" userwavefile="" latt="0" sustain="0.5" lamt="0" lshp="0" lspd_denominator="4" lspd_numerator="4" x100="0" rel="0.1" dec="0.5" att="0"/>
                  <elres lspd="0.1" ctlenvamt="0" lpdel="0" pdel="0" amt="0" hold="0.5" syncmode="0" userwavefile="" latt="0" sustain="0.5" lamt="0" lshp="0" lspd_denominator="4" lspd_numerator="4" x100="0" rel="0.1" dec="0.5" att="0"/>
                </eldata>
                <chordcreator chordrange="1" chord="0" chord-enabled="0"/>
                <arpeggiator arpdir="0" arpgate="100" arptime_denominator="4" syncmode="0" arp-enabled="0" arprange="1" arptime_numerator="4" arpmode="0" arp="0" arptime="100"/>
                <midiport inputchannel="0" fixedinputvelocity="-1" outputcontroller="0" outputchannel="1" fixedoutputvelocity="-1" readable="0" fixedoutputnote="-1" outputprogram="1" writable="0" basevelocity="127" inputcontroller="0"/>
                <fxchain numofeffects="0" enabled="0"/>
              </instrumenttrack>
              <pattern type="0" muted="0" steps="16" name="Hat_o.ds" pos="0" len="192"/>
            </track>
            <track type="0" muted="0" name="Kick.ds" solo="0">
              <instrumenttrack pitch="0" vol="100" fxch="1" pan="0" basenote="57" usemasterpitch="1" pitchrange="1">
                <instrument name="audiofileprocessor">
                  <audiofileprocessor interp="1" reversed="0" looped="0" sframe="0" lframe="0" eframe="1" src="drumsynth/cr8000/Kick.ds" amp="100" stutter="0"/>
                </instrument>
                <eldata fwet="0" ftype="0" fres="0.5" fcut="14000">
                  <elvol lspd="0.1" ctlenvamt="0" lpdel="0" pdel="0" amt="0" hold="0.5" syncmode="0" userwavefile="" latt="0" sustain="0.5" lamt="0" lshp="0" lspd_denominator="4" lspd_numerator="4" x100="0" rel="0.1" dec="0.5" att="0"/>
                  <elcut lspd="0.1" ctlenvamt="0" lpdel="0" pdel="0" amt="0" hold="0.5" syncmode="0" userwavefile="" latt="0" sustain="0.5" lamt="0" lshp="0" lspd_denominator="4" lspd_numerator="4" x100="0" rel="0.1" dec="0.5" att="0"/>
                  <elres lspd="0.1" ctlenvamt="0" lpdel="0" pdel="0" amt="0" hold="0.5" syncmode="0" userwavefile="" latt="0" sustain="0.5" lamt="0" lshp="0" lspd_denominator="4" lspd_numerator="4" x100="0" rel="0.1" dec="0.5" att="0"/>
                </eldata>
                <chordcreator chordrange="1" chord="0" chord-enabled="0"/>
                <arpeggiator arpdir="0" arpgate="100" arptime_denominator="4" syncmode="0" arp-enabled="0" arprange="1" arptime_numerator="4" arpmode="0" arp="0" arptime="100"/>
                <midiport inputchannel="0" fixedinputvelocity="-1" outputcontroller="0" outputchannel="1" fixedoutputvelocity="-1" readable="0" fixedoutputnote="-1" outputprogram="1" writable="0" basevelocity="127" inputcontroller="0"/>
                <fxchain numofeffects="0" enabled="0"/>
              </instrumenttrack>
              <pattern type="0" muted="0" steps="16" name="Kick.ds" pos="0" len="192"/>
            </track>
            <track type="0" muted="0" name="Rim.ds" solo="0">
              <instrumenttrack pitch="0" vol="100" fxch="1" pan="0" basenote="57" usemasterpitch="1" pitchrange="1">
                <instrument name="audiofileprocessor">
                  <audiofileprocessor interp="1" reversed="0" looped="0" sframe="0" lframe="0" eframe="1" src="drumsynth/cr8000/Rim.ds" amp="100" stutter="0"/>
                </instrument>
                <eldata fwet="0" ftype="0" fres="0.5" fcut="14000">
                  <elvol lspd="0.1" ctlenvamt="0" lpdel="0" pdel="0" amt="0" hold="0.5" syncmode="0" userwavefile="" latt="0" sustain="0.5" lamt="0" lshp="0" lspd_denominator="4" lspd_numerator="4" x100="0" rel="0.1" dec="0.5" att="0"/>
                  <elcut lspd="0.1" ctlenvamt="0" lpdel="0" pdel="0" amt="0" hold="0.5" syncmode="0" userwavefile="" latt="0" sustain="0.5" lamt="0" lshp="0" lspd_denominator="4" lspd_numerator="4" x100="0" rel="0.1" dec="0.5" att="0"/>
                  <elres lspd="0.1" ctlenvamt="0" lpdel="0" pdel="0" amt="0" hold="0.5" syncmode="0" userwavefile="" latt="0" sustain="0.5" lamt="0" lshp="0" lspd_denominator="4" lspd_numerator="4" x100="0" rel="0.1" dec="0.5" att="0"/>
                </eldata>
                <chordcreator chordrange="1" chord="0" chord-enabled="0"/>
                <arpeggiator arpdir="0" arpgate="100" arptime_denominator="4" syncmode="0" arp-enabled="0" arprange="1" arptime_numerator="4" arpmode="0" arp="0" arptime="100"/>
                <midiport inputchannel="0" fixedinputvelocity="-1" outputcontroller="0" outputchannel="1" fixedoutputvelocity="-1" readable="0" fixedoutputnote="-1" outputprogram="1" writable="0" basevelocity="127" inputcontroller="0"/>
                <fxchain numofeffects="0" enabled="0"/>
              </instrumenttrack>
              <pattern type="0" muted="0" steps="16" name="Rim.ds" pos="0" len="192"/>
            </track>
            <track type="0" muted="0" name="Snare.ds" solo="0">
              <instrumenttrack pitch="0" vol="100" fxch="1" pan="0" basenote="57" usemasterpitch="1" pitchrange="1">
                <instrument name="audiofileprocessor">
                  <audiofileprocessor interp="1" reversed="0" looped="0" sframe="0" lframe="0" eframe="1" src="drumsynth/cr8000/Snare.ds" amp="100" stutter="0"/>
                </instrument>
                <eldata fwet="0" ftype="0" fres="0.5" fcut="14000">
                  <elvol lspd="0.1" ctlenvamt="0" lpdel="0" pdel="0" amt="0" hold="0.5" syncmode="0" userwavefile="" latt="0" sustain="0.5" lamt="0" lshp="0" lspd_denominator="4" lspd_numerator="4" x100="0" rel="0.1" dec="0.5" att="0"/>
                  <elcut lspd="0.1" ctlenvamt="0" lpdel="0" pdel="0" amt="0" hold="0.5" syncmode="0" userwavefile="" latt="0" sustain="0.5" lamt="0" lshp="0" lspd_denominator="4" lspd_numerator="4" x100="0" rel="0.1" dec="0.5" att="0"/>
                  <elres lspd="0.1" ctlenvamt="0" lpdel="0" pdel="0" amt="0" hold="0.5" syncmode="0" userwavefile="" latt="0" sustain="0.5" lamt="0" lshp="0" lspd_denominator="4" lspd_numerator="4" x100="0" rel="0.1" dec="0.5" att="0"/>
                </eldata>
                <chordcreator chordrange="1" chord="0" chord-enabled="0"/>
                <arpeggiator arpdir="0" arpgate="100" arptime_denominator="4" syncmode="0" arp-enabled="0" arprange="1" arptime_numerator="4" arpmode="0" arp="0" arptime="100"/>
                <midiport inputchannel="0" fixedinputvelocity="-1" outputcontroller="0" outputchannel="1" fixedoutputvelocity="-1" readable="0" fixedoutputnote="-1" outputprogram="1" writable="0" basevelocity="127" inputcontroller="0"/>
                <fxchain numofeffects="0" enabled="0"/>
              </instrumenttrack>
              <pattern type="0" muted="0" steps="16" name="Snare.ds" pos="0" len="192"/>
            </track>
          </trackcontainer>
        </bbtrack>
      </track>
    </trackcontainer>
    <track type="6" muted="0" name="Automation track" solo="0">
      <automationtrack/>
      <automationpattern prog="0" mute="0" name="Numerator" pos="0" tens="1" len="192"/>
      <automationpattern prog="0" mute="0" name="Denominator" pos="0" tens="1" len="192"/>
      <automationpattern prog="0" mute="0" name="Tempo" pos="0" tens="1" len="192"/>
      <automationpattern prog="0" mute="0" name="Master volume" pos="0" tens="1" len="192"/>
      <automationpattern prog="0" mute="0" name="Master pitch" pos="0" tens="1" len="192"/>
      <automationpattern prog="0" mute="0" name="Numerator" pos="0" tens="1" len="192"/>
      <automationpattern prog="0" mute="0" name="Denominator" pos="0" tens="1" len="192"/>
      <automationpattern prog="0" mute="0" name="Tempo" pos="0" tens="1" len="192"/>
      <automationpattern prog="0" mute="0" name="Master volume" pos="0" tens="1" len="192"/>
      <automationpattern prog="0" mute="0" name="Master pitch" pos="0" tens="1" len="192"/>
      <automationpattern prog="0" mute="0" name="Numerator" pos="0" tens="1" len="192"/>
      <automationpattern prog="0" mute="0" name="Denominator" pos="0" tens="1" len="192"/>
      <automationpattern prog="0" mute="0" name="Tempo" pos="0" tens="1" len="192"/>
      <automationpattern prog="0" mute="0" name="Master volume" pos="0" tens="1" len="192"/>
      <automationpattern prog="0" mute="0" name="Master pitch" pos="0" tens="1" len="192"/>
    </track>
    <fxmixer visible="1" width="561" height="332" x="10" y="314" maximized="0" minimized="0">
      <fxchannel num="0" muted="0" volume="1" name="Master" soloed="0">
        <fxchain numofeffects="0" enabled="0"/>
      </fxchannel>
      <fxchannel num="1" muted="0" volume="0.4" name="cr8000" soloed="0">
        <fxchain numofeffects="0" enabled="0"/>
        <send amount="1" channel="0"/>
      </fxchannel>
    </fxmixer>
    <ControllerRackView visible="1" width="258" height="142" x="608" y="307" maximized="0" minimized="0"/>
    <pianoroll visible="0" width="640" height="480" x="1" y="200" maximized="0" minimized="0"/>
    <automationeditor visible="0" width="640" height="400" x="56" y="255" maximized="0" minimized="0"/>
    <projectnotes visible="0" width="640" height="400" x="683" y="1" maximized="0" minimized="0"><![CDATA[<!DOCTYPE HTML PUBLIC "-//W3C//DTD HTML 4.0//EN" "http://www.w3.org/TR/REC-html40/strict.dtd">
<html><head><meta name="qrichtext" content="1" /><style type="text/css">
p, li { white-space: pre-wrap; }
</style></head><body style=" font-family:'Verdana'; font-size:11pt; font-weight:600; font-style:normal;">
<p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;"><span style=" font-family:'Sans Serif'; font-size:9pt; font-weight:400; color:#e0e0e0;">Put down your project notes here.</span></p></body></html>]]></projectnotes>
    <timeline lp0pos="0" lp1pos="192" lpstate="0"/>
    <controllers/>
  </song>
</lmms-project>
