FreeMat: YLIM Adjust Y Axis limits of plot

FreeMat

- Main Page
- Related Pages

YLIM Adjust Y Axis limits of plot

Section: Handle-Based Graphics

# Usage

There are several ways to use `ylim` to adjust the Y axis limits of a plot. The various syntaxes are

       ylim
       ylim([lo,hi])
       ylim('auto')
       ylim('manual')
       ylim('mode')
       ylim(handle,...)

The first form (without arguments), returns a 2-vector containing the current limits. The second form sets the limits on the plot to `[lo,hi]`. The third and fourth form set the mode for the limit to `auto` and `manual` respectively. In `auto` mode, FreeMat chooses the range for the axis automatically. The `ylim('mode')` form returns the current mode for the axis (either `'auto'` or `'manual'`). Finally, you can specify the handle of an axis to manipulate instead of using the current one.

As an additional feature, you can now specify `inf` for a limit, and FreeMat will take that limit from the automatic set. So, for example `ylim([10,inf])` will set the minimum for the y axis, but use the automatic value for the maximum.

# Example

    --> x = linspace(-1,1);
    --> y = sin(2*pi*x);
    --> plot(x,y,'r-');
    --> ylim  % what are the current limits?

    ans =
       -0.9999    0.9999

which results in

Next, we zoom in on the plot using the `ylim` function

    --> plot(x,y,'r-')
    --> ylim([-0.2,0.2])

which results in

To demonstrate the infinite limits feature. Consider the following

    --> plot(x,y,'r-');
    --> ylim([0,inf])

which results in